[Information]
; (Latest Translator, First Translator, Second Translator ...)
TRANSLATOR=منتديات عميد التعريب   _   الأستاذ عوض الغامدي
VERSION=4.5.0

[Language]
LANGUAGE= عربي 
CHARACTER_CODE=Unicode (UTF-16, LE, w/ BOM)
; Local ID : http://msdn.microsoft.com/en-us/library/ms912047(WinEmbedded.10).aspx
LOCALE_ID=0x1401,0x3C01,0x0C01,0x0801,0x2C01,0x3401,0x3001,0x1001,0x1801,0x2001,0x4001,0x0401,0x2801,0x1C01,0x3801,0x2401

[Url]
WIKIPEDIA_SMART=https://en.wikipedia.org/wiki/Self-Monitoring,_Analysis_and_Reporting_Technology

[Menu]
FILE=&ملف
CUSTOMIZE=ت&خصيص
EXIT=&خروج
EDIT=ت&حرير
COPY=&نسخ
FUNCTION=ال&وظيفة
HIDE_SMART_INFO=&S.M.A.R.T. إخفاء معلومات
HIDE_SERIAL_NUMBER=إخفاء &رقم التسلسل
SHOW_DRIVE_LETTER=إظهار &حرف محرك القرص
ADVANCED_DISK_SEARCH=بحث &متقدم في القرص
EVENT_LOG=&سجل الحدث
AAM_APM_CONTROL=AA&M/APM تحكم
AUTO_AAM_APM_ADAPTION=آلية AAM/A&PM ملاءمة
RESIDENT=أيقونة &جوار الساعة
STARTUP=&بدء التشغيل
OPEN_DISK_MANAGEMENT="فتح "&إدارة الأقراص
OPEN_DEVICE_MANAGER="فتح "&إدارة الأجهزة
ADVANCED_FEATURE=ميزة &متقدمة
REFRESH=&تحديث
RESCAN=إ&عادة فحص
DISABLE=ت&عطيل
AUTO_REFRESH=تحديث تلقا&ئي
AUTO_REFRESH_TARGET=&هدف التحديث التلقائي
AUTO_REFRESH_TARGET_ALL_DISK=التحديث التلقائي - إ&ستهداف كافة الأقراص
AUTO_REFRESH_UNTARGET_ALL_DISK=التحديث التلقائي - &عدم إستهداف كافة الأقراص
WAIT_TIME_AT_STARTUP=وقت الإ&نتظار عند بدء التشغيل
GRAPH=&رسم بياني
THEME=&سمات
DISK=ال&قرص
HELP=تعل&يمات
HELP_WEB=&Օգնություն [Web]
HELP_ABOUT=ترجمة الأستاذ عوض الغامدي
HELP_ABOUT_SMART=زيارة منتديات عميد التعريب
LANGUAGE=ال&لغة
ITEM=ال&مادة
TEMPERATURE_TYPE=&نوع الحرارة
CELSIUS=(°C) مئوية
FAHRENHEIT=(°F) فهرنهايت
HEALTH_STATUS_SETTING=إ&عداد حالة السلامة

;Graph
OPTION=&خيارات
LEGEND_POSITION=مكان &التوضيح
NORTH_WEST=ال&شمال الغربي
NORTH_EAST=الشمال الش&رقي
SOUTH_WEST=الجنوب ال&غربي
SOUTH_EAST=الج&نوب الشرقي
MAX_PLOT_POINT=أ&قصى نقطة للحبكة
TIME_FORMAT=&صيغة الوقت
PAINT_WEEKEND=ألوان نهاية الأ&سبوع
ALL=ال&كل

;2.7.0
COPY_OPTION=&خيار النسخ
RESIDENT_STYLE=&عند الإغلاق
MINIMIZE=تصغير
HIDE=إخفاء

;3.0.0
ZOOM=ال&بؤرة
AUTO=&تلقائية
ATTRIBUTE=ال&خاصية

;3.5.0
ASCII_VIEW=ASCII عرض
AUTO_DTECTION=إكتشاف آلي
SECOND=ثانية
MINUTE=دقيقة
HOUR=ساعة

:3.9.4
WORKAROUND=&حل بديل

;4.0.0
ALERT_MAIL=البريد للتنبيه
MAIL_SETTINGS=إعدادات البريد
SMART_IN_ENGLISH=بالإنجليزية S.M.A.R.T.
FONT_SETTING=إعداد الخطوط

;5.0.0
ALERT_FEATURES=A&lert Features
ALARM_HISTORY=Alarm History
ALERT_SOUND=Alert Sound
SOUND_SETTINGS=Sound Settings
GADGET_SUPPORT=Gadget Support
INSTALL_GADGET=Install Gadget
ENABLE_AUTO=Enable (Auto Detection)
ENABLE_ALL=Enable (All Disks)
ENABLE_RAID=Enable (RAID Volume Only)

;6.0.0
HIDE_NO_SMART_DISK=&Hide No S.M.A.R.T. Disk
GREEN_MODE=&Green Mode

;8.6.0
SAVE_TEXT=Save (&text)
SAVE_IMAGE=&Save (image)

;9.0.0
DRIVE_SORT_METHOD=Drive Sort Method
PHYSICAL_DRIVE_ID=Physical Drive ID
DRIVE_LETTER=Drive Letter

;9.2.0
VOICE=Voice

;9.3.0
STARTUP_VOICE=Startup Voice

;9.5.0
HIDE_RAID_VOLUME=Hide &RAID Volume
[TrayMenu]
EXIT=خروج
REFRESH=تحديث
RESCAN=إعادة فحص
ENABLE=تمكين
DISABLE=تعطيل
ENABLE_ALL=تمكين الكل
DISABLE_ALL=تعطيل الكل
AUTO_REFRESH=تحديث تلقائي
AUTO_REFRESH_01_MIN=دقيقة
AUTO_REFRESH_03_MIN=3 دقائق
AUTO_REFRESH_05_MIN=5 دقائق
AUTO_REFRESH_10_MIN=10 دقائق
AUTO_REFRESH_30_MIN=30 دقيقة
AUTO_REFRESH_60_MIN=60 دقيقة
AUTO_REFRESH_TARGET=هدف التحديث التلقائي
AUTO_REFRESH_TARGET_ALL_DISK=التحديث التلقائي - إستهداف كافة الأقراص
AUTO_REFRESH_UNTARGET_ALL_DISK=التحديث التلقائي - عدم إستهداف كافة الأقراص
ALARM_SETTING_TEMPERATURE=إعداد المنبه - الحرارة
ALARM_SETTING_HEALTH_STATUS=إعداد المنبه - حالة السلامة
SHOW_MAIN_WINDOW=إظهار النافذة الرئيسية
SHOW_TEMPERATURE_ICON=إظهار أيقونة درجة الحرارة
SHOW_ALL_TEMPERATURE_ICON=إظهار أيقونة لكافة درجات الحرارة
HIDE_ALL_TEMPERATURE_ICON=إخفاء أيقونة لكافة درجات الحرارة
COLLECTIVE_SETTING=إعداد جماعي
GRAPH=مخطط بياني
;Added 3.0
SHOW_TEMPERATURE_ICON_ONLY=إظهار أيقونة الحرارة فقط

[DiskStatus]
GOOD=جيدة
CAUTION=تحذير
BAD=سيئة
UNKNOWN=غير معروفة
DISK=القرص

[Dialog]
LIST_ID=الهوية
LIST_CURRENT=الحالي
LIST_WORST=سيئة جدا
LIST_THRESHOLD=العتبة
LIST_RAW_VALUES=قيم خام
;LIST_DESCRIPTION=الوصف
LIST_ATTRIBUTE_NAME=إسم الخاصية

FIRMWARE=البرنامج الداخلي
SERIAL_NUMBER=رقم التسلسل
INTERFACE=الواجهة
STANDARD=عادي
TRANSFER_MODE=نمط النقل
BUFFER_SIZE=حجم المخزون المؤقت
NV_CACHE_SIZE=المؤقت NV حجم مخزون
ROTATION_RATE=معدل الدوران
TEMPERATURE=الحرارة
POWER_ON_HOURS=ساعات توصيل التيار
POWER_ON_COUNT=عدد مرات توصيل التيار
DRIVE_LETTER=حرف القرص
FEATURE=المميزات المعتمدة
HEALTH_STATUS=حالة القرص

UNKNOWN=غير معروفة
POWER_ON_COUNT_UNIT=مرة
POWER_ON_HOURS_UNIT=ساعة
POWER_ON_DAYS_UNIT=يوم
POWER_ON_YEARS_UNIT=سنوات

;4.3
TOTAL_HOST_WRITES=Host إجمالي عدد عمليات كتابة
TOTAL_HOST_READS=Host إجمالي عدد عمليات قراءة
TOTAL_NAND_WRITES=NAND عمليات كتابة

;4.5
WEAR_LEVELING_COUNT=مرات تسوية الطبقة الخارجية

;6.1
CURRENT_MODE_SUPPORTED_MODE=Current Mode | Supported Mode
MAJOR_VERSION_MINOR_VERSION=Major Version | Minor Version

;8.5.0
FONT_FACE=Font Face
FONT_SCALE=Font Scale (%)
DEFAULT=Default

;8.9.0
ENABLED=Enabled
DISABLED=Disabled

[Message]
DETECT_UNIT_POWER_ON_HOURS=إكتشاف وحدة "ساعات توصيل التيار" (تتطلب حوالي 130 ثانية) ـ
DETECT_DISK=إكتشاف القرص
PLEASE_ENABLE_WMI=(Windows إدارة أجهزة) WMI الرجاء تمكين
PLEASE_RESTART_THIS_APPLICATION=الرجاء إعادة تشغيل التطبيق من أجل تغيير السمة
DISK_NOT_FOUND=القرص غير موجود

[Alarm]
ALARM_TEMPERATURE=المنبه - درجة الحرارة
ALARM_HEALTH_STATUS=المنبه - حالة السلامة
DEGRADATION=تخفيض الطاقة
RECOVERY=الإسترداد
;3.5.0
INFO_HEALTH_STATUS=معلومات - حالة السلامة	

[Graph]
PLEASE_SELECT_ITEM=الرجاء تحديد مادة
ACTUAL_VALUE=(القيمة الفعلية (القيمة الخام
NORMALIZED_VALUE=(القيمة الطبيعية (القيمة الحالية
ALL_ON=الكل شغال
ALL_OFF=الكل إغلاق
RESET=إعادة الوضع

[Customize]
LINE_COLOR=لون السطر
BACKGROUND_IMAGE=صورة الخلفية
SUPPORTED_IMAGE_FORMAT=صيغة الصورة المعتمدة
ALL_FILES=كافة الملفات

;5.0.0
SUPPORTED_SOUND_FORMAT=Supported Sound Format

[AamApm]
AAM_LOW=<- (80h) صامت
AAM_HIGH=الأداء (FEh) ->
AAM_RECOMMEND=القيمة المستحسنة
APM_LOW=<- (01h) أدنى طاقة
APM_HIGH=الأداء (FEh) ->
;3.5.0
AUTOMATIC_ACOUSTIC_MANAGEMENT=(AAM) الإدارة الصوتية الآلية
ADVANCED_POWER_MANAGEMENT=(APM) إدارة الطاقة المتقدمة

[WindowTitle]
ABOUT=حول
GRAPH=مخطط بياني
CUSTOMIZE=تخصيص
VERSION_INFORMATION=معلومات الإصدار
AAM_APM_CONTROL=AAM/APM تحكم
HEALTH_STATUS_SETTING=إعداد حالة السلامة

;5.0.0
ALARM_HISTORY=Alarm History
SOUND_SETTINGS=Sound Settings

;5.1.0
FONT_SETTING=إعداد الخطوط

[HealthStatus]
THRESHOLD_OF_CAUTION=عتبة التحذير
APPLY=تطبيق
DEFAULT=الإفتراضي

[Smart]
UNKNOWN=غير معروفة
VENDOR_SPECIFIC=بائع معين
01=معدل خطأ القراءة
02=أداء الإنتاجية
03=وقت الدوران
04=غدد مرات البدء/الإيقاف
05=عدد القطاعات المعاد تخصيصها
06=قراءة هامش القناة
07=معدل تقصي الخطأ
08=أداء وقت التقصي
09=ساعات توصيل الطاقة
0A=عدد محاولات التدوير
0B=محاولة إعادة ضبط المعايرة
0C=عدد دورات الطاقة
0D=محاولة معدل الخطأ الناعم للقراءة
B8=End-to-End خطأ
BB=الأخطاء الغير قابلة للتصحيح في التقرير
BC=نفاذ الوقت لسطر الأوامر
BD=High Fly كتابة
BE=درجة حرارة إندفاع الهواء
BF=G-Sense معدل خطأ
C0=عدد تراجع إغلاق الطاقة
C1=عدد تحميل/عدم تحميل الدورة
C2=الحرارة
C3=المستردة ECC أجهزة
C4=عدد الحدث لإعادة التخصيص
C5=عدد القطاعات المعلقة حاليا
C6=عدد القطاعات الغير قابلة للتصحيح
C7=UltraDMA CRC عدد أخطاء
C8=معدل الخطأ للكتابة
C9=Soft معدل خطأ قراءة
CA=خطأ في علامة عنوان البيانات
CB=إلغاء نفاذ التشغيل
CC=ناعم ECC تصحيح
CD=معدل قسوة الحرارية
CE=إرتفاع التحليق
CF=التيار العالي للدوران
D0=طنين الدوران
D1=أداء التقصي بغير إتصال
D3=الإهتزاز أثناء القراءة
D4=النتر أثناء الكتابة
DC=تبديل القرص
DD=G-Sense معدل خطأ
DE=الساعات المحملة
DF=عدد محاولات التحميل/عدم التحميل
E0=إحتكاك التحميل
E1=عدد تحميل/عدم تحميل الدورة
E2='In'-تحميل وقت
E3=عدد توسع الطوق
E4=فصل الطاقة عن دورة التقهقر
E6=GMR إتساع مقدمة
E7=الحرارة
F0=ساعات تحليق المقدمة
FA=معدل محاولات خطأ القراءة
FE=حماية حرة كاملة

;Updated 5.4.0
F1=المكتوبة LBA إجمالي
F2=المقروءة LBA إجمالي

;Updated 9.5.0
17=Helium Condition Lower
18=Helium Condition Upper
1B=MAMR Health Monitor

[SmartSsd]
01=معدل خطأ القراءة
02=أداء الإنتاجية
03=وقت الدوران
04=غدد مرات البدء/الإيقاف
05=عدد القطاعات المعاد تخصيصها
06=قراءة هامش القناة
07=معدل تقصي الخطأ
08=أداء وقت التقصي
09=ساعات توصيل الطاقة
0A=عدد محاولات التدوير
0B=محاولة إعادة ضبط المعايرة
0C=عدد دورات الطاقة
0D=محاولة معدل الخطأ الناعم للقراءة
C0=عدد مرات الإغلاق المفاجيء
C2=الحرارة
C4=عدد الحدث لإعادة التخصيص
C5=عدد القطاعات المعلقة حاليا
C6=عدد القطاعات الغير قابلة للتصحيح
; CrystalDiskInfo assign
FF=الحياة المتبقية

;Updated 5.4.0
F1=Total Host Writes
F2=Total Host Reads

[SmartMtron]
BB=عدد المحو الكلي

[SmartIndilinx]
01=معدل خطأ القراءة
09=ساعات توصيل الطاقة
0C=عدد دورات الطاقة
B8=عدد تهيئة الكتل السيئة
C3=عدد كتل البرنامج الفاشلة
C4=عدد كتل المحو الفاشلة
C5=عدد كتل القراءة الفاشلة
C6=العدد الكلي لقطاعات القراءة
C7=العدد الكلي لقطاعات الكتابة
C8=العدد الكلي لأوامر القراءة
C9=العدد الكلي لأوامر الكتابة
CA=FLASH من Bit العدد الكلي لأخطاء
CB=القابلة للتصحيح Bit العدد الكلي لقطاعات القراءة مع أخطاء
CC=معلمة الكتلة السيئة الكاملة
CD=PE مواصفات أقصى عدد لـ
CE=أدنى عدد للمحو
CF=أقصى عدد للمحو
D0=متوسط عدد المحو
D1=حياة القرص المتبقية

[SmartJMicron60x]
09=ساعات توصيل الطاقة
0C=عدد دورات الطاقة
C2=الحرارة
E5=Flash هوية إنهيار النظام , هوية
E8=نسخة البرنامج الداخلي
E9=مؤشر هدر الوسائط
EA=متوسط عدد المحو , أقصى عدد للمحو
EB=عدد الكتل الجيدة , عدد كتل النظام

[SmartIntel]
03=وقت التسارع
04=غدد مرات البدء/الإيقاف
05=عدد القطاعات المعاد تخصيصها
09=عدد ساعات توصيل الطاقة
0C=عدد دورات الطاقة
C0=عدد مرات الإغلاق المفاجيء
E1=عمليات كتابة المضيف
E8=المساحة المحجوزة المتوفرة
E9=مؤشر تلاشي الوسيطة
B8=في التقرير I/O أخطاء الرمز في كشف أخطاء

;Updated 4.1
AA=المساحة المحجوزة المتوفرة
AB=عدد مرات فشل البرنامج
AC=عدد مرات فشل المحو
BB=عدد الأخطاء الغير قابلة للتصحيح

;Updated 4.3
AE=مرات فقدان الطاقة المغاجئ
E2=التأثير اللحظي لتشغيل الوسيطة
E3=Host معدل التشغيل الزمني للكتابة/للقراءة
E4=المؤقت للتشغيل الزمني
F1=المكتوبة LBA إجمالي
F2=المقروءة LB&A إجمالي
F9=NAND عمليات كتابة

;Updated 5.5.0
B7=SATA Downshift Count
BE=Temperature
C7=CRC Error Count

;Updated 5.6.1
AF=Power Loss Protection Failure
C2=Temperature
C5=Pending Sector Count

;Added 6.6.0
EA=Thermal Throttle Status

[SmartSamsung]
05=عدد القطاعات المعاد تخصيصها
09=ساعات توصيل الطاقة
0C=عدد مرات توصيل الطاقة
AF=(عدد مرات فشل البرنامج (رقاقة
B0=(عدد فشل المحو (رقاقة
B1=مرات تسوية الطبقة الخارجية
B2=(عدد الكتل المحجوزة المستخدمة (رقاقة
B3=(عدد الكتل المحجوزة المستخدمة (المجموع
B4=(عدد الكتل المحجوزة الغير مستخدمة (المجموع
B5=(عدد مرات فشل البرنامج (الكلي
B6=عدد مرات فشل المحو
B7=(زمن التشغيل للكتل السيئة (الكلي
BB=عدد الأخطاء الغير قابلة للتصحيح
BE=درجة حرارة إندفاع الهواء
C2=الحرارة
C3=ECC معدل خطأ
C6=عدد الأخطاء بدون الإتصال غير قابلة للتصحيح
C7=CRC عدد أخطاء
C9=Super cap حالة
CA=SSD حالة وضعية
EB=POR عدد مرات إسترداد
F1=المكتوبة LBA إجمالي
F2=المقروءة LBA إجمالي

;Added 6.6
AA=Unused Reserved Block Count (Chip) 
AB=Program Fail Count (Chip)
AC=Erase Fail Count (Chip)
AD=Wear Leveling Count
AE=Unexpected Power Loss Count
B8=Error Detection
E9=Normalized Media Wear-out

[SmartSandForce] ;Updated (3.7)
01=Raw Read معدل الخطأ
05=عدد الكتل العاطلة
09=ساعات توصيل الطاقة
0C=عدد دورات الطاقة
0D=Soft معدل خطأ قراءة
64=الغيغابايت الممسوحة
AA=عدد الكتل المحجوزة
AB=عدد مرات فشل البرنامج
AC=عدد مرات فشل المحو
AE=مرات فقدان الطاقة المغاجئ
B1=نطاق إرتداء دلتا
B5=عدد مرات فشل البرنامج
B6=عدد مرات فشل المحو
B8=في التقرير I/O أخطاء الرمز في كشف أخطاء
BB=الأخطاء الغير قابلة للتصحيح في التقرير
C2=الحرارة
C3=الغير قابلة للتصحيح On‐the‐Fly ECC أخطاء
C4=عدد الحدث لإعادة التخصيص
C6=عدد القطاعات الغير قابلة للتصحيح
C7=SATA R- أخطاء (CRC) عدد أخطاء
C9=معدل الخطأ للقراءة السلسة الغير متوافقة
CC=Soft ECC معدل تصحيح
E6=وضع منحنى العمر
E7=المتبقي SSD عمر
E8=المساحة المحجوزة المتوفرة
EB=SuperCap سلامة
F1=من المستضيف Lifetime مرات كتابة
F2=القراءات مدى العمر من المضيف

[SmartJMicron61x] ;Added (3.9)
01=Raw Read معدل قراءة
02=أداء الإنتاجية
03=وقت الدوران
05=عدد القطاعات المعاد تخصيصها
07=معدل تقصي الخطأ
08=أداء وقت التقصي
09=ساعات توصيل الطاقة
0A=عدد محاولات التدوير
0C=عدد دورات الطاقة
A8=SATA PHY عدد أخطاء
AF=(عدد فشل البرنامج (الرقاقة
C0=مرات فقدان الطاقة المغاجئ
C2=الحرارة
C5=عدد القطاعات المعلقة حاليا
AA=عدد الكتل السيئة
AD=مرات المحو

[SmartMicron] ;Added 4.0.0/ Updated 6.1.0
; RAIN = Redundant Array of Independent NAND
01=Raw Read معدل الخطأ
05=عدد القطاعات المعاد تخصيصها
09=ساعات توصيل الطاقة
0C=عدد دورات الطاقة
AB=عدد مرات فشل البرنامج
AC=عدد مرات فشل المحو
AE=مرات فقدان الطاقة المغاجئ
B7=SATA تدهور واجهة
BB=الأخطاء الغير قابلة للتصحيح في التقرير
BD=عدد الكتل السيئة التصنيع
C4=عدد الحدث لإعادة التخصيص
C5=عدد القطاعات المعلقة حاليا
C6=الغير قابل للتصحيح Smart Off-line عدد أخطاء فحص
C7=Ultra DMA CRC معدل الخطأ لـ
CE=معدل الخطأ للكتابة
F2=تقدم الحماية ضد الكتابة

;4.5
B8=عدد مرات تصحيح الأخطاء
C2=الجرارة الباطنية
C3=التراكمية المصححة ECC عدد

;5.6.0
0D=Soft Error Rate
AA=Reserved Block Count
AD=Average Block-Erase Count
BC=Command Timeout Count
CA=Percent Lifetime Used

;6.0.0
0E=Device Capacity (NAND)
0F=User Capacity
10=Spare Blocks Available
11=Remaining Spare Blocks
64=Total Erase Count
B4=Unused Reserve NAND Blocks
B5=Unaligned Access Count
D2=Successful RAIN Recovery Count
EA=Total Bytes Read
F2=Write Protect Progress
F3=ECC Bits Corrected
F4=ECC Cumulative Threshold Events
F5=Cumulative Program NAND Pages
F6=Total Host Sector Writes
F7=Host Program Page Count
F8=FTL Program Page Count

[SmartMicronMU02] ;Updated 6.6.0
; RAIN = Redundant Array of Independent NAND
01=Raw Read Error Rate
05=Reallocated Sectors Count
09=Power-On Hours
0C=Power Cycle Count
0D=Soft Error Rate
0E=Device Capacity (NAND)
0F=User Capacity
10=Spare Blocks Available
11=Remaining Spare Blocks
64=Total Erase Count
AA=Reserved Block Count
AB=Program Fail Count
AC=Erase Fail Count
AD=Average Block-Erase Count
AE=Unexpected Power Loss Count
B4=Unused Reserve NAND Blocks
B7=SATA Interface Downshift
B8=Error Correction Count
BB=Reported Uncorrectable Errors
BC=Command Timeout Count
BD=Factory Bad Block Count
C2=Temperature
C3=Cumulative ECC Bit Correction Count
C4=Reallocation Event Count
C5=Current Pending Sector Count
C6=Smart Off-line Scan Uncorrectable Error Count
C7=Ultra DMA CRC Error Rate
CA=Percent Lifetime Used
CE=Write Error Rate
D2=Successful RAIN Recovery Count
EA=Total Bytes Read
F3=ECC Bits Corrected
F4=ECC Cumulative Threshold Events
F5=Cumulative Program NAND Pages
F6=Total Host Sector Writes
F7=Host Program Page Count
F8=Background Program Page Count

; Updated 6.6.0
A0=Uncorrectable Sector Count
A1=Valid Spare Blocks
A3=Initial Invalid Blocks
94=Total SLC Erase Count
95=Maximum SLC Erase Count
96=Minimum SLC Erase Count
97=Average SLC Erase Count
A4=Total TLC Erase Count
A5=Maximum TLC Erase Count
A6=Minimum TLC Erase Count
A7=Average TLC Erase Count
A9=Percentage Lifetime Remaining
B5=Program Fail Count
B6=Erase Fail Count
C0=Power-off Retract Count
E8=Available Reserved Space
F1=Total LBA Write
F2=Total LBA Read
F5=Total TLC Write Count
F6=Total SLC Write Count
F7=RAID Recovery Count

[SmartOcz] ;Added (4.5)
01=معدل أخطاء القراءة الأولية
03=وقت التسارع
04=مرات التشغيل و التوقف
05=عدد القطاعات المعاد تخصيصها
09=ساعات توصيل الطاقة
0C=مرات تدوير الطاقة
E8=إجمالي العدد لقطاعات الكتابة
E9=عمر القرص المتبقي

; Added 6.6.0
64=Total Blocks Erased
A7=SSD Protect Mode
A8=SATA PHY Error Count
A9=Bad Block Count
AD=Erase Count
B8=Factory Bad Block Count
C0=Unexpected Power Loss Count
CA=Total Number of Corrected Bits
CD=Max Rated PE Counts
CE=Minimum Erase Counts
CF=Maximum Erase Counts
D3=SATA Uncorrectable Error Count
D4=NAND Page Reads During Retry
D5=Simple Read Retry Attempts
D6=Adaptive Read Retry Attempts
DD=Internal Data Path Uncorrectable Errors
DE=RAID Recovery Count
E6=Power Loss Protection
FB=NAND Read Count

;Updated 6.7.0
F1=Total Host Writes
F2=Total Host Reads

[SmartPlextor] ;Added (5.1.0)/Updated (5.4.0)
01=Read Error Rate
05=Reallocated Sectors Count
09=Power-On Hours
0C=Power Cycle Count
AA=Grown Bad Blocks
AB=Program Fail Count
AC=Erase Fail Count
AD=Average Program/Erase Count
AE=Unexpected Power Loss Count
AF=Program Fail Count (Worst Case)
B0=Erase Fail Count (Worst Case)
B1=Wear Leveling Count
B2=Used Reserved Block Count (Worst Case)
B3=Used Reserved Block Count
B4=UnUsed Reserved Block Count (Total)
B5=Program Fail Count
B6=Erase Fail Count
B7=SATA Interface Down Shift
B8=End-to-End Data Errors Corrected
BB=Uncorrectable Error Count
BC=Command Time out
C0=Unsafe Shutdown Count
C3=ECC rate
C4=Reallocation Event Count
C6=Uncorrectable Sector Count
C7=Ultra CRC Error Count
E8=Available Reserved Space
E9=NAND GB written
F1=Total Host Writes
F2=Total Host Reads

[SmartSanDisk] ;Added (5.2.0)
05=Retired Block Count
09=Power-On Hours
0C=Power Cycle Count
AA=Reserve Block Count
AB=Program Fail Count
AC=Erase Fail Count
AE=Unexpected Power Loss Count
BB=Reported Uncorrectable Errors
E8=Remaining Life
F1=Total Host Writes
F2=Total Host Reads

[SmartOczVector] ;Added (5.3.0)
05=Accumulated Runtime Bad Blocks
09=Power-On Hours Count
0C=Power Cycle Count
AB=Available Over-Provisioned Block Count
AE=Power Cycle Count (Unplanned)
BB=Total Uncorrectable NAND Reads
C3=Total Programming Failures
C4=Total Erase Failures
C5=Total Read Failures (Uncorrectable)
C6=Host Reads
C7=Host Writes
D0=Average Erase Count
D2=SATA CRC Error Count
E9=Remaining Life
F9=Total NAND Programming Count

;Updated 5.5.0
F1=Total Host Writes
F2=Total Host Reads

;Updated 6.6.0
64=Total Blocks Erased
B8=Factory Bad Block Count Total
CA=Total Number Of Read Bits Corrected
CD=Max Rated PE Count
CE=Min Erase Count
CF=Max Erase Count
D4=Total Count NAND Pages Reads Requiring Read Retry
D5=Total Count of Simple Read Retry Attempts
D6=Total Count of Adaptive Read Retry Attempts
DD=Internal Data Path Protection Uncorrectable Errors
DE=RAID Recovery Count
E0=In Warranty
E1=DAS Polarity
E2=Partial Pfail
E6=Write Throttling Activation Flag
F9=Total NAND Programming Count (pages)
FB=Total NAND Read Count

[SmartCorsair] ;Added 6.2.0
01=Raw Read Error Rate
05=Retired Block Count
09=Power On Hours
0C=Power Cycle Count
AA=Reserve Block Count
AC=Erase Fail Count
AE=Unexpected Power Loss Count
B5=Program Fail Count
BB=Reported Uncorrectable Errors
C2=Temperature
C4=Reallocation Event Count
E7=SSD Life Left
F1=Lifetime GB Written
F2=Lifetime GB Read

[SmartToshiba] ;Added 6.2.0
01=Read Error Rate
02=Throughput Performance
03=Spin-Up Time
04=Start/Stop Count
05=Reallocated Sectors Count
07=Seek Error Rate
08=Seek Time Performance
09=Power-On Hours
0A=Spin Retry Count
0B=Recalibration Retries
0C=Power Cycle Count
A7=SSD Protect Mode
A8=SATA PHY Error Count
A9=Total Bad Block Count
AD=Erase Count
C0=Unexpected Power Loss Count
C2=Temperature
C4=Reallocation Event Count
C5=Current Pending Sector Count
C6=Uncorrectable Sector Count
F1=Total Host Writes
F2=Total Host Reads

[SmartSanDiskGb] ;Added 6.2.0
05=Reallocated Block Count
09=Power On Hours
0C=Power Cycle Count
A6=Min W/E Cycle
A7=Max Bad Block/Die
A8=Maximum Erase Cycle
A9=Total Bad Block
AB=Program Fail Count
AC=Erase Fail Count
AD=Average Erase Cycle
AE=Unexpected Power Loss Count
BB=Reported Uncorrectable Errors
C2=Temperature
D4=SATA PHY Error
E6=Percentage Total P/E Count
E8=Spare Block Remaining
E9=Total GB Written To NAND
F1=Total GB Written
F2=Total GB Read

[SmartKingston] ;Added 6.6.0
01=Read Error Rate
02=Throughput Performance
03=Spin Up Time
05=Reallocated Sectors Count
07=Seek Error Rate
08=Seek Time Performance
09=Power-On Hours
0A=Spin Retry Count
0C=Power Cycle Count
A8=SATA PHY Error Count
AA=Bad Block Count
AD=Erase count
AF=Bad Cluster Table Count
BB=Uncorrectable Errors
C0=Unsafe Shutdown Count
C2=Temperature
C4=Later Bad Block Count
C5=Current Pending Sector Count
C7=CRC Error Count
DA=CRC Error Count
E7=SSD Life Left
E9=Lifetime Writes to Flash
F0=Write Head
F1=Host Writes
F2=Host Reads
F4=Average Erase Count
F5=Max Erase Count
F6=Total Erase Count

[SmartNVMe] ;Added 6.7.0
01=Critical Warning
02=Composite Temperature
03=Available Spare
04=Available Spare Threshold
05=Percentage Used
06=Data Units Read
07=Data Units Written
08=Host Read Commands
09=Host Write Commands
0A=Controller Busy Time
0B=Power Cycles
0C=Power On Hours
0D=Unsafe Shutdowns
0E=Media and Data Integrity Errors
0F=Number of Error Information Log Entries

[SmartRealtek] ;Added by Realtek
01=Raw data error rate
05=Reallocated sector count
09=Power on hour count
0C=Power cycle count
A1=GDN
A2=Total erase count
A3=Max PE cycle
A4=Average erase count
A5=Initial bad block count
A6=Total bad block count
A7=SSD protect mode
A8=SATA Phy error count
A9=Health
AB=Program fail count
AC=Erase fail count
AE=Unexpected power loss count
AF=ECC fail count
B5=Unaligned access count
BB=Reported uncorrectable error
C2=Enclosure temperature
C3=Cumulative corrected ecc
C4=Reallocation event count
C7=Ultra DMA CRC error count
CE=Min. erase count
CF=Max erase count
E7=Lifetime left
E8=Available reserved space
F1=Write life time
F2=Read life time
F9=Total GB written to NAND (TLC)
FA=Total GB written to NAND (SLC)

[SmartSKhynix] ; Updated 8.8.0
01=Read Error Rate
05=Re-Assigned Sector Count
09=Power-On Hours
0C=Power Cycle Count
64=Total Erase Count
A8=Min. Erase Count
A9=Max. Erase Count
AA=Reserve Block Count
AB=Program Fail Count
AC=Erase Fail Count
AE=Unexpected Power Loss Count
AF=Program Fail Count(Worst Case)
B0=Erase Fail Count(Worst Case)
B1=Wear Leveling Count
B2=Used Reseved Block Count(Worst Case)
B3=Used Reseved Block Count(SSD Total)
B4=UnUsed Reseved Block Count(SSD Total)
B5=Program Fail Count(SSD Total)
B6=Erase Fail Count(SSD Total)
B7=SATA Downshift Count
B8=End-to-End Error Detection Count
BB=Uncorrectable Error Count
BC=Command Timeout Count
BF=Op Shock Event Count
C2=Temperature
C3=ECC Rate
C4=Reallocation Event Count
C6=Uncorrectable Sector Count
C7=CRC Error Count
C9=Uncorrectable Soft Read Error Rate
CC=Soft ECC Correction Rate
D4=Phy Error Count
E7=SSD Life Left
E9=SSD Life Left
EA=NAND Written
F1=Total LBA Written
F2=Total LBA Read
FA=Total Number of NAND Read Retries

[SmartKioxia]
09=Power-On Hours Count
0C=Device Power Cycle Count
A7=SSD Protect Mode
A8=SATA PHY Error Count
A9=Bad Block Count
AD=Erase Count (User Data)
C0=Unexpected Power Loss Count
C2=Temperature
F1=Host Writes

[SmartWdc]
01=Read Error Rate
05=Reassigned Block Count
09=Power On Hours
0C=Power Cycle Count
A5=Block Erase Count (SLC)
A6=Minimum P/E Cycles
A7=Maximum Bad Blocks per die
A8=Maximum P/E Cycles
A9=Total Bad Block
AA=Grown Bad Blocks
AB=Program Fail Count
AC=Erase Fail Count
AD=Average P/E Cycles
AE=Unexpected Power Loss Count
B8=End-to-End Error Detection/Correction Count
BB=Reported Uncorrectable Errors
BC=Command Timeout Count
C2=Temperature
C7=CRC Error Count
D4=SATA PHY Error
E6=Media Wearout Indicator
E8=Available Reserve Space
E9=NAND GB Written
EA=NAND GB Written (SLC)
EE=Media Wearout Indicator (Cycles Remaining)
F1=Total GB Written
F2=Total GB Read
F4=Temperature Throttle Status
F9=NAND GB Written

[SmartKingstonSuv]
01=Read Error Rate
05=Reallocated Sector Count
09=Power On Hours
0C=Power Cycle Count
AA=Used Reserved Block Count
AB=Program Fail Count
AC=Erase Fail Count
AE=Unexpected Power Off Count
AF=Program Fail Count Worst Die
B0=Erase Fail Count Worst Die
B1=Wear Leveling Count
B2=Used Reserved Block Count worst Die
B4=Unused Reserved Block Count (SSD Total)
BB=Reported Uncorrectable Errors
C2=Temperature
C3=On-the-Fly ECC Error Count
C4=Reallocation Event Count
C5=Pending Sector Count
C7=UDMA CRC Error Count
C9=Uncorrectable Read Error Rate
CC=Soft ECC Correction Rate
E7=SSD Life Left
EA=Lifetime Nand Writes
F1=Lifetime Host Writes
F2=Lifetime Host Reads
FA=Total Number of NAND Read Retries

[SmartKingstonKC600]
01=Read Error Rate
05=Re-Allocated NAND Block Count
09=Power-On Hours
0C=Power Cycle Count
94=Reserved
95=Reserved
96=Reserved
97=SLC Average Erase Count
9F=DRAM 1 bit Error Count
A0=Reported UECC (UnCorrectable) Errors
A1=Available Reserved Space
A4=Reserved
A5=Reserved
A6=Reserved
A7=Average Erase Count
A8=Reserved
A9=Percentage Of Rated Lifetime Remaining
B1=Reserved
B5=Program Fail Count
B6=Erase Fail Count
C0=Unexpected Power Loss Count
C2=Device Temperature
C3=Hardware ECC Recovered
C4=Reallocation Event Count
C7=UDMA CRC Error Count
E7=Percentage of Rated Lifetime Remaining
E8=Unused Reserved Block Count
F1=Total LBAs Written
F2=Total LBAs Read
F5=Total Media Writes

[SmartKingstonDC500]
01=Host UNC Error Count
09=Power on Hours
0C=Power On / Off Cycle
A7=Protect mode
A8=SATA PHY Error Count
A9=Bad Block Rate
AA=Bad Block Information
AC=Erase Failure Count
AD=Erase Count
B5=Program Fail Count
B6=Erase Failure Count
BB=Host UNC Error Count
C0=Unexpected Power Loss Count
C2=Temperature
C4=Total Later Bad Block Count
C7=CRC Error Count
CF=Thermal Throttling Count
DA=CRC Error Count
E7=SSD Life Remaining
E8=Read Fail Count
E9=NAND Write
F1=Host Write
F2=Host Read
F4=Avg Erase Count
F5=Max Erase Count
F6=Total Erase Count

[SmartKingstonSA400]
01=Uncorrectable Errors
09=Power On Hours
0C=Power Cycles
94=Vendor Unique
95=Vendor Unique
A7=Vendor Unique
A8=SATA PHY Error Count
A9=Vendor Unique
AA=Bad Block Count
AC=Vendor Unique
AD=Erase Count
B5=Vendor Unique
B6=Vendor Unique
BB=Uncorrectable ECC Errors
C2=Temperature
C4=Reallocation Events
C7=SATA CRC Error
DA=CRC Error Count
E7=SSD Wear Indicator
E9=Lifetime Nand Writes
F1=Lifetime Writes from Host
F2=Lifetime Read from Host
F4=Average Erase Count
F5=Max Erase Count
F6=Total Erase Count

[SmartSsstc]
01=Raw Read Error Rate
05=Reallocated Block Count
09=Power On Hours
0C=Power Cycle Count
AA=Available Reserved Space
AB=Program Fail Count(Total)
AC=Erase Fail Count(Total)
AD=Average Program/Erase Count
AE=Unexpected Power Loss Count
AF=Program Fail count (Worst case)
B0=Erase Fail Count (Worst case)
B1=Wear Leveling Count
B2=Used Reserved Block Count (Worst case)
B3=Used Reserved Block Count (Total)
B4=Unused Reserved Block Count (Total)
B7=SATA Interface Down shift
B8=End-to-End Data Errors Count
BB=Uncorrectable Error Count
BC=Command Time out
C2=Drive Temperature
C3=ECC rate
C6=OffLine Uncorrectable Error Count
C7=SATA CRC Error Count
E5=Power Loss Protection Failure
E7=Percentage Lifetime Remaining
E8=Available Reserved Space 
E9=NAND GB Written
F1=Total Host Write
F2=Total Host Read 
F3=NAND GB Written

[SmartIntelDc]
01=Raw Read Error Count
05=Reallocated Flash Block Count
09=Power-On Hours Count
0C=Power Cycle Count
0E=Device Capacity
0F=User Capacity
10=Spare Blocks Available
11=Remaining Spare Available
AC=Total Block Erase Failure
AD=Per Block Max Erase Count
AE=Unexpected Power Loss Count
AF=Average Erase Count
B0=Power Loss Protection Error
B5=Total Block Program Failure
B8=End-to-End Error Detection Count
BB=Uncorrectable Error Count
C2=Temperature
C5=Pending Sector Count
C6=Offline Uncorrectable Error Count
C7=CRC Error Count
CA=Percentage of Drive Life Used
E2=Timed Workload - Media Wear
E3=Timed Workload - Host Read/Write Ratio
E4=Timed Workload Timer
EA=Total Host Bytes Read
EB=Total Host Bytes/Sectors Written
F1=Total Nand Bytes/Sectors Written

[SmartApacer]
09=Power on Hours
0C=Power Cycle Count
A3=Maximum Erase Count
A4=Average Erase Count
A6=Total Later Bad Block Count
A7=SSD Protect Mode
A8=SATA PHY Error Count
AB=Program Fail Count
AC=Erase Fail Count
AF=Bad Cluster Table Count
C0=Unexpected Power Loss Count
C2=Temperature
E7=Lifetime Left
F1=Total Sectors Write

[SmartSiliconMotion]
01=Read Error Rate
05=Reallocated Sectors Count
09=Power-On Hours
0C=Power Cycle Count
94=SLC Total Erase Count
95=SLC Maximum Erase Count
96=SLC Minimum Erase Count
97=SLC Average Erase Count
9F=DRAM 1 bit Error Count
A0=Uncorrectable sectors count when read/write
A1=Number of Valid Spare Blocks
A2=Number of Cache Data Block
A3=Number of Initial Invalid Blocks
A4=Total Erase Count
A5=Maximum Erase Count
A6=Minimum Erase Count
A7=Average Erase Count
A8=Max Erase Count of Spec
A9=Remain Life
AF=Program fail count in worst die
B0=Erase fail count in worst die
B1=Total Wear Level Count
B2=Runtime Invalid Block Count
B5=Total Program Fail Count
B6=Total Erase Fail Count
BB=Uncorrectable Error Count
C0=Power-Off Retract Count
C2=Temperature
C3=Hardware ECC Recovered
C4=Reallocation Event Count
C5=Current Pending Sector Count
C6=Uncorrectable Error Count Off-line
C7=Ultra DMA CRC Error Count
E8=Available Reserved Space
F1=Total LBA Written
F2=Total LBA Read
F5=Flash Write Sector Count

[SmartJMicron66x]
01=Read Error Rate
02=Throughput Performance
03=Spin-Up Time
05=Reallocated Sectors Count
07=Seek Error Rate
08=Seek Time Performance
09=Power-On Hours
0A=Spin Retry Count
0C=Power Cycle Count
A8=SATA PHY Error Count
AA=Bad Block Count
AD=Erase Count
AF=Bad Cluster Table Count
B4=Spare Block Count
C0=Unexpected Power Loss Count
C2=Temperature
C5=Current Pending Sector Count
E7=Drive Life
E9=Write Sector Count (NAND)
F0=Write Head
F1=Total LBA Written
F2=Total LBA Read

[SmartPhison]
01=Read Error Rate
09=Power on Hours
0C=Power Cycle Count
A8=SATA PHY Error Count
AA=Bad Block Count
AD=Erase Count
C0=Unexpected Power Loss Count
C2=Temperature
DA=Number of CRC Error
E7=SSD Life Left
F1=Host Writes

[SmartSeagate]
01=Read Error Rate
05=Retired Sectors Count
09=Power On Hours
0C=Power Cycle Count
10=Spare Blocks Available
11=Remaining Spare Blocks
A8=SATA PHY Error Count
AA=Bad Block Count
AB=Program Fail Count
AC=Erase Fail Count
AD=Erase Count
AE=Unexpected Power Loss Count
B1=Wear Range Delta
B5=Program Fail Count
B6=Erase Fail Count
C0=Unexpected Power loss Count
C2=Temperature
C9=Soft Error Rate
CC=Soft ECC Correction Rate
DA=CRC Error Count
E7=SSD Life Left
E8=Read Failure Block Count
E9=NAND GiB Written
EA=Lifetime Writes To Flash
EB=NAND sectors Written
F1=Lifetime Writes From Host
F2=Lifetime Reads From Host
FA=Lifetime NAND Read Retries

[SmartSeagateIronWolf]
01=Raw Read Error Rate
05=Reallocated Sector Count
09=Power On Hours
0C=Power Cycle Count
64=Flash Gigabytes Erased
66=Lifetime PS4 Entry Count
67=Lifetime PS3 Entry Count
AA=Grown Bad Block Count
AB=Program Fail Count
AC=Erase Fail Count
AD=Average Program/Erase Count
AE=Unexpected Power Loss Count
B1=Wear Range Delta
B7=SATA/PCIe Interface Downshift Count
BB=Uncorrectable ECC Count
C2=Temperature
C3=RAISE ECC Correctable Count
C6=Uncorrectable Read Error Count
C7=SATA R-Error (CRC) Error Count
E6=Drive Life Protection Status
E7=SSD Life Left
E8=Available Reserved Space
E9=Lifetime Writes to Flash
F1=Lifetime Writes From Host
F2=Lifetime Reads From Host
F3=Free Space

[SmartMarvell] ; Added 8.8.3
05=Number of New Bad Block
09=Power On Hours
0C=Power Cycle Count
A4=Total Erase Count
A5=Maximum Erase Count
A6=Minimum Erase Count
A7=Average Erase Count
C0=Power off Retract Count
C2=Temperature
C7=SATA CRC Error Count
F1=Total Written
F2=Total Read

[SmartMaxiotek] ; Added 8.8.6
05=Reallocated Sector Count
09=Power-On Hours
0C=Drive Power Cycle Count
A7=SSD Protect Mode
A8=PHY Error Count
A9=Bad Block Count
AB=Program Fail Count
AC=Erase Fail Count
AD=Erase Count
AF=Bad Cluster Table Count
B1=Read Retry Count
B4=Spare Block Count Left
BB=Reported UNC Errors
C0=Unexpected Power Loss Count
C2=Temperature
C4=Reallocated Event Count
C7=UDMA CRC Error Count
CE=Minimum Erase Count
CF=Maximum Erase Count
D0=Average Erase Count
D1=Minimum Erase Count of SLC block
D2=Maximum Erase Count of SLC block
D3=Average Erase Count of SLC block
E7=SSD Life Left
E9=Write Counts Sectors to Nand
EA=Read Counts Sectors from Nand
F1=Write Sector Count
F2=Read Sector Count
F5=Bit Error Count

[SmartSeagateBarraCuda] ; Added 8.9.0
01=UECC Error Count
05=Retired Sectors Count
09=Power On Hours
0C=Power Cycle Count
10=Spare Blocks Available
11=Remaining Spare Blocks
A8=SATA PHY Error Count
AA=Bad Block Count
AB=Program Fail Count
AC=Erase Fail Count
AD=Erase Count
AE=Unexpected Power Loss Count
B1=Wear Range Delta
B5=Program Fail Count
B6=Erase Fail Count
C0=Unexpected Power loss Count
C2=Temperature
C9=Soft Error Rate
CC=Soft ECC Correction Rate
DA=CRC Error Count
E7=SSD Life Left
E8=Read Failure Block Count
E9=NAND GiB Written
EA=Lifetime Writes To Flash
EB=NAND sectors Written
F1=Lifetime Writes From Host
F2=Lifetime Reads From Host
FA=Lifetime NAND Read Retries

[SmartYmtc] ; Added 8.10.0
05=New Bad Block Count
09=Power-On Hours Count
0C=Power Cycle Count
AA=Max Bad Block Count
A8=SATA PHY Error Count
A9=Bad Block Count
AB=Program Fail Count
AC=Erase Fail Count
AD=Erase Count
AF=Bad Cluster Count
B7=SATA Interface Downshift
B8=End to End Error Detection/Correction Count
BB=Uncorrectable Error Count
BE=Temperature
C0=Unexpected Power Loss Count
C4=Re-allocated Event Count
C7=CRC Error Count
CE=Minimum Erase Count
CF=Maximum Erase Count
D0=Average Erase Count
D1=SLC Minimum Erase Count
D2=SLC Maximum Erase Count
D3=SLC Average Erase Count
E7=SSD Life Left
E9=Write sector count to NAND
EA=Read sector count to NAND
F1=Total LBA written
F2=Total LBA Read
F3=NAND Temperature
F5=Bit Error Count

[SmartScy] ;Added 8.12.8
01=Raw Read Error Rate
05=Reallocated Sector Count
07=Seek Error Rate
09=Power-On Hours
0C=Drive Power Cycle Count
A7=Average Erase Count
AB=Program Fail Count
AC=Erase Fail Count
AD=Erase Count
B1=Read Retry Count
B4=Spare Block Count Left
B7=Runtime Bad Block
BB=Reported UNC Errors
C0=Unexpected Power Loss Count
C2=Controlled Temperature
C3=Cumulative ECC Bit Correction Count
C4=Reallocated Event Count
C5=Current Pending Sector
C7=UDMA CRC Error Count
E7=SSD Life Left
F1=Total LBAs Written
F2=Total LBAs Read
F5=Total Nand Flash Written

[SmartRecadata] ;Added 8.14.0
07=Seek Error Rate
09=Power-On Hours
0C=Drive Power Cycle Count
A7=Average erase count
AB=Program Fail Count
AC=Erase Fail Count
AD=Erase Count
B1=Read Retry Count
B4=Spare Block Count Left
B7=Runtime Bad Block
BB=Reported UNC Errors
C0=Unexpected Power Loss Count
C2=Controlled temperature
C3=Cumulative ECC Bit Correction Count
C4=Reallocated Event Count
C5=Current Pending Sector
C7=UDMA CRC Error Count
E7=SSD Life Left
F1=Total LBAs written
F2=Total LBAs read
F5=Total Nand Flash Written

[SmartSanDiskHp] ;Added 8.17.0
01=Raw Read Error Rate
05=Reassigned Block Count
09=Power On Hours
0C=Drive Power Cycle Count
AA=Reserved Block Count
AB=Program Fail Count
AC=Erase Fail Count
AD=Wear Leveling Count
AE=Unexpected Power Loss Count
B0=Unused Reserved Block Count
B7=SATA Interface Downshift Count
B8=End to End Error Detection/Correction Count
BB=Uncorrectable Error Count
BC=Command Time Out
BE=Airflow Temperature
C2=Temperature
C4=Reallocated Event Count
C7=CRC Error Count
C9=SSD Life Left
E6=Media Wearout Indicator
F1=Total LBAs Written
F2=Total LBAs Read
F3=Throttle Statistics
F4=Temperature Throttle Status
F9=TLC NAND GB Writes

[SmartSanDiskHpVenus] ;Added 8.17.0
01=Raw Read Error Rate
05=Reassigned Block Count
09=Power On Hours
0C=Drive Power Cycle Count
AA=Reserved Block Count
AB=Program Fail Count
AC=Erase Fail Count
AD=Wear Leveling Count
AE=Unexpected Power Loss Count
B0=Unused Reserved Block Count
B7=SATA Interface Downshift Count
B8=End to End Error Detection/Correction Count
BB=Uncorrectable Error Count
BC=Command Time Out
BE=Airflow Temperature
C2=Temperature
C4=Reallocated Event Count
C7=CRC Error Count
C9=SSD Life Left
E6=Media Wearout Indicator
F1=Total LBAs Written
F2=Total LBAs Read
F3=Total NAND Writes
F4=Temperature Throttle Status
F9=TLC NAND GB Writes

[SmartSanDiskDell] ;Added 8.17.0
05=Reassigned Block Count
09=Power On Hours
0C=Drive Power Cycle Count
AF=Program Fail Count (Worst Case Component)
B0=Erase Fail Count (Worst Case Component)
B1=Wear Leveling Count
B2=Used Reserved Block Count (Worst Case Component)
B3=Used Reserved Block Count (SSD Total)
B4=Remaining Reserved Block Count (SSD Total)
B5=Program Fail Count (SSD Total)
B6=Erase Fail Count (SSD Total)
BB=Uncorrectable Error Count
C2=Temperature
C3=ECC Rate
C7=CRC Error Count
E6=Media Wearout Indicator
EE=Media Wearout Indicator (Cycles Remaining)
F1=Total LBAs Written
F2=Total LBAs Read

[SmartSanDiskLenovo] ;Added 8.17.0
05=Reassigned Block Count
09=Power On Hours
0C=Drive Power Cycle Count
A6=Minimum P/E Cycles
A7=Maximum Bad Blocks per Die
A8=Maximum P/E cycles
A9=Total Bad Blocks
AA=Grown Bad Blocks
AB=Program Fail Count
AC=Erase Fail Count
AD=Average P/E Cycles Attribute
AE=Unexpected Power Loss Count
B2=Used Reserved Block Count
B4=Remaining Reserved Block Count
B8=End to End Error Detection/Correction Count
BB=UECC Count
BC=Command Time Out
C2=Temperature
C7=SATA CRC Errors
D4=SATA PHY Errors
E6=Media Wearout Indicator
E8=Available Reserved Space
E9=NAND GB Written
EA=NAND GB Written (SLC)
F1=Total Host GB Write
F2=Total GB Read
F3=Throttle Statistics
F4=Thermal Throttle Status

[SmartSanDiskLenovoHelenVenus] ;Added 8.17.0
05=Reassigned Block Count
09=Power On Hours
0C=Drive Power Cycle Count
A6=Minimum P/E Cycles
A7=Maximum Bad Blocks per Die
A8=Maximum P/E cycles
A9=Total Bad Blocks
AA=Grown Bad Blocks
AB=Program Fail Count
AC=Erase Fail Count
AD=Average P/E Cycles Attribute
AE=Unexpected Power Loss Count
B2=Used Reserved Block Count
B4=Remaining Reserved Block Count
B8=End to End Error Detection/Correction Count
BB=UECC Count
BC=Command Time Out
C2=Temperature
C7=SATA CRC Errors
D4=SATA PHY Errors
E8=Available Reserved Space
E9=Media Wearout Indicator
EA=NAND GB Written (SLC)
F1=Total Host GB Write
F2=Total GB Read
F3=Throttle Statistics
F4=Thermal Throttle Status
F9=NAND GB Written (TLC)

[SmartMicronMU03] ;Added 8.17.0
01=Raw Read Error Rate
05=Reallocated NAND Block Count
09=Power On Hours Count
0C=Power Cycle Count
AB=Program Fail Count
AC=Erase Fail Count
AD=Average Block Erase Count
AE=Unexpected Power Loss Count
B4=Unused Spare NAND Blocks
B5=Non-4K Aligned Access
B7=SATA interface Downshift
B8=Error Correction Count
BB=Reported Uncorrectable Errors
C2=Temperature
C4=Reallocation Event Count
C5=Current Pending ECC Count
C6=SMART Offline Scan Uncorrectable Error Count
C7=UDMA CRC Error Count
CA=Lifetime Remaining
CE=Write Error Rate
D2=Successful RAIN Recovery Count
F0=Host Program Page Count
F1=Total LBAs Written
F2=Total LBAs Read
F3=Total Program Page Count
F6=Cumulative Host Sectors Written
F7=Host Program NAND Pages Count
F8=FTL Program NAND Pages Count

[SmartSanDiskCloud] ;Added 9.0.0
05=Retired Block Count
09=Power On Hours
0D=Count of Uncorrectable ECC Errors
20=Write Amplification multiplied by 100
21=Write Amplification Factor
AA=Reserve Block Count
AB=Program Fail Count
AC=Erase Fail Count
AD=Average Write/Erase Count
AE=Unexpected Power Loss Count
B2=SSD Life Left (upto 0.01%)
BF=Clean Shutdown Count
C0=Unclean Shutdown Count
C2=Temperature
C4=Number of Blocks Reallocated
E6=Percent of Total Write/Erase Count
E8=Spare Blocks Remaining
E9=Total Nand Writes 64GB
EB=Capacitor Health
F1=Total Host Writes 64GB
F2=Total Host Reads 64GB
F4=Lifetime Thermal Throttle Activations
F5=Percent Drive Life Remaining
FD=SPI Tests Remaining

[SmartSiliconMotionCVC] ;Added 9.3.0
05=Re-Assigned Count
09=Power-On Hours Count
0C=Drive Power Cycle Count
A5=SLC Cache
AA=Grown Bad Block Count
AB=Program Fail Count
AC=Erase Fail Count
AD=Avg Erase Count
AE=Unexpected Power Loss Count
AF=Program Fail Count (Worst case)
B7=Total SATA Link Speed Downshift
B8=End-to-End Data Errors corrected
BB=Uncorrectable Errors
BD=Max Erase Count
BE=Temperature
BF=Min Erase Count
C3=Read Error Rate
C6=Off-Line Scan Uncorrectable Sector Count
C7=SATA CRC Error Count
CA=SSD Life Left
E8=Total Spare Counts
E9=TLC NAND Write
F1=Host Write
F2=Host Read
94=RAID Event Count
95=RAID Uncorrectable Count
A7=SSD Protect Mode
93=Soft Retry Event Count
EA=SLC NAND Write

[SmartAdataIndustrial] ;Added 9.3.1
09=Power-On hours Count
0C=Drive Power Cycle Count
A7=SSD Protect Mode
A8=SATA PHY Error Count
A9=Bad Block Count
AD=Erase Count
AF=Bad Cluster Table Count
B4=Spare block count left
C0=Unexpected Power Loss Count
C2=Temperature
E7=SSD life left
E9=Flash Write Sector Count
EA=Flash Read Sector Count
F1=Write Sector Count
F2=Read Sector Count
